|  |
| --- |
|  |

**Moulded Connectors**

**The ALS moulded connectors are available in the full range of FAA style connectors, and can be manufactured in any length or combination.**

**Compliance:**

All ALS Moulded connectors meet the following

industry standards:

FAA A/C 150-5345-26D - Plug and Socket Design

**Features:**

• Manufactured from high quality TPE.

• Full range of plugs and sockets available

• Interchangeable with any other manufacturers’

plug and sockets

• Ambient temperature range -55°C to +65°C

• Resistant to acid and alkaline soils, oils, fuels and

de-icing fluids

**Applications:**

• Custom made extension leads

• Alternative to onsite connector kit